**DERBYDOG INC**

**DEMOLITION DERBY**

**2023 WINDSHIELD CLASS**

**2/3/2023**

**QUESTIONS? TEXT:**

-JEREMY HEJDUK (440)-223-4723

**MINIS/VANS:** 1980 & newer front-wheel drive, sub-frame automobile. Maximum 6 cylinder

**FULL-SIZE:** Any 1980 & newer automobile is permitted. No leaf spring cars permitted.

-Windshield optional to be removed. All other glass must be removed

-No drivetrain swaps permitted. Must be drivetrain for make/model of vehicle used.

-Battery may be relocated to inside car

-Fuel tank may be relocated to back seat area or left in stock location

-Rear seat bar permitted (Maximum 2”). No downlegs. NO OTHER WELDING PERMITTED ANYWHERE (except where noted)!

-All doors, hood, decklid MUST be wired, chained, or banded shut

-Bumpers may be bolted on. A 2” wide x 2” long strapping may be used to weld on top of frame to bumper. Bumper must be factory production appearing bumper for car. No bumper swaps! **NO AFTERMARKET BUMPERS!** OFFICIALS DECISION IS FINAL!

-Street tires ONLY! Factory production wheels D.O.T. 4-PLY MAX.!

-Headers permitted.

-Pre-ran cars are permitted. No added welding anywhere! If bumper tears off, bumper may be re-mounted in above welded manner. No shortening of front frame except where damaged.

**No Fixit Plates permitted PERIOD. CHEAP!! EASY!! FUN!!**

**-CHEAP! EASY! FUN! Don’t ruin it for everyone else PLEASE!**